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Shanghai Koyo -Anp Import & Export Co., Ltd        


1. CGI Sheet; 一年的采购数量：101,760
	Material photos
	Sr
	Specification
	Unit
	Remark

	Corrugated Iron Galvanized Iron sheet (CGI) Zinc coated iron sheet
波纹镀锌屋面板
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	1
	Material: Iron sheet with corrugated and Galvanizing of Zinc by Hot Dipping-coating (Galvanized Steel Sheet-G90)

材质：波形钢板热镀锌镀锌（镀锌钢板-G90）
	Minimum 0.90 oz of Zinc per square-feet of coating

每平方英尺涂层最少0.90盎司锌
	Intl/local manufacture norm (G90)

国际/本地制造标准（G90）

	
	2
	Base Sheet Thickness: 
30 Gauge: 0.3 mm or 0.012 inch

Tolerance: +/- 0.05mm

Tensile: High tensile steel

底板厚度：

30规格：0.3毫米或0.012英寸

公差：+/- 0.05mm

拉伸：高强度钢
	Gauge, millimeter
Minimum 550 Mpa strength

尺寸，毫米

最低550Mpa的强度
	AWG/BWG

	
	3
	Coating Thickness: Code G90 
Thickness per side

Top: 18µm; Back: 5-8µm

涂层厚度：G90

每边厚度

上：18μm; 背面：5-8μm
	0.45oz per square-feet in both sides coating micron unit for thickness
每平方英尺0.45盎司双面涂层微米单位的厚度
	ASTM A653

	
	4
	Corrugated profile 11 nos, Waves
Pitch-slope: 76mm approx

Depth-height: 18mm approx

Tolerance: +/- 2 mm

波纹状的轮廓11号，波浪？
斜坡：约76毫米

深度 - 高度：约18毫米

公差：+/- 2毫米
	Qty of corrugated peaks Dimension in millimeter (or inch)
波峰单位为毫米（或英寸）
	Intl/local manufacture norm
国际/本地制造规范

	
	5
	Size of sheet: Width2.5 Feet (762 mm); Length: 7 Feet (2133mm) minimum (Tolerance width ±4mm, length ±15mm)
板材尺寸：宽度2.5英尺（762毫米）; 长度：最小7英尺（2133mm）（公差宽度±4mm，长度±15mm）
	Feet/inch or Meter/millimeter 
英尺/英寸或米/毫米
	Intl/local manufacture norm
国际/本地制造规范

	
	6
	Single sheet weight: 2.5 kg minimum Tolerance +/- 2%
单张重量：至少2.5千克，最小容差+/- 2％
	Kilogram or (Ton in bulk)
千克或（吨散装）
	Intl/local manufacture norm
国际/本地制造规范

	
	7
	Sheet Hardness HRB: 85HRB minimum
板材硬度HRB：最低85HRB
	Brinell Hardness Number. An abbreviation: e.g. 85 HRB
布氏硬度值。 缩写：例如 85 HRB
	International norm
国际制造规范

	
	8
	Prefer standard: JIS G 3302-1987 or local standard/code
首选标准：JIS G 3302-1987或当地标准/规范
	Refer to Japan Industry Standard
参照日本工业标准
	International norm
国际制造规范

	Stamping Profiles
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Note1: Standard wire gauges of American Wire Gauge: AWG, Birmingham Wire Gauge: BWG

Note2: The similar profile in Zinc coated, galvanized sheet and Aluminium- Zinc coated sheet

90 Galvanized Steel is hot dipped in zinc – coated with a minimum 0.90 oz. of zinc per square foot. Mean apply 0.45oz. of zinc to each side total of 0.45x2=0.90 oz

1：美国线规的标准线规：AWG，伯明翰线规：BWG

2：镀锌，镀锌板和镀铝锌板的类似外形

90镀锌钢热浸镀锌，最低0.90盎司镀锌/平方英尺。 平均值为0.45oz 锌每边总计0.45×2 = 0.90盎司

2. Alu-Zinc coated Types，一年的采购数量：101,760
	Material photos
	Sr
	Specification
	Unit
	Remark

	Corrugated Iron sheet with Aluminium- Zinc coating
铝锌涂层波纹屋面板
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	1
	Material: Iron sheet with corrugated and Dipping-coating by Aluminum-Zinc compound (Zinc alume: AZ150)
材料：波纹铝板和铝锌合金（Zincalume：AZ150）
	Minimum Zincalume 150 gram per square meter of Coating
至少每平方米涂层150克锌渣
	Intl/local manufacture norm (AZ150)
国际/本地制造标准（AZ150）

	
	2
	Base Sheet Thickness: 
30 Gauge: 0.3 mm or 0.012 inch

Tolerance: +/- 0.05mm

Tensile: High tensile steel
底板厚度：

30规格：0.3毫米或0.012英寸

公差：+/- 0.05mm

拉伸：高强度钢
	Gauge, millimeter
Minimum 550 Mpa strength
尺寸，毫米

最低550Mpa的强度
	AWG/BWG

	
	3
	Coating Thickness: Code AZ150

Thickness per side

Top: 18µm; Back: 5-8µm
涂层厚度：代码AZ150

每边厚度

上：18μm; 背面：5-8μm
	75gm per square meter in both sides coating micron unit for thickness
两面涂层微米单位厚度为每平方米75克
	ASTM A653
ASTM A653

	
	4
	Corrugated profile 11 nos, Waves

Pitch-slope: 76mm approx

Depth-height: 18mm approx

Tolerance: +/- 2 mm
波纹状的轮廓为11号，波浪 ？
斜坡：约76毫米

深度 - 高度：约18毫米

公差：+/- 2毫米
	Qty of corrugated peaks Dimension in millimeter (or inch)
波峰单位为毫米（或英寸）
	Intl/local manufacture norm
国际/本地制造规范

	
	5
	Size of sheet: Width2.5 Feet (762 mm);
 Length: 7 Feet (2133mm) minimum (Tolerance width ±4mm, length ±15mm)
板材尺寸：宽度2.5英尺（762毫米）; 长度：最小7英尺（2133mm）（公差宽度±4mm，长度±15mm）
	Feet/inch or Meter/millimeter 
英尺/英寸或米/毫米
	Intl/local manufacture norm
国际/本地制造规范

	
	6
	Single sheet weight: () kg minimum Tolerance +/- 2%
单张重量：（kg）最小值公差+/- 2％
	Kilogram or (Ton in bulk)

千克或（吨散装）
	Intl/local manufacture norm
国际/本地制造规范

	
	7
	Sheet Hardness HRB: 85HRB minimum

板材硬度HRB：最低85HRB
	Brinell Hardness Number. An abbreviation: e.g. 85 HRB

布氏硬度值。 缩写：例如 85 HRB
	International norm

国际制造规范

	
	8
	Prefer standard: JIS G 3302-1987 or local standard/code

首选标准：JIS G 3302-1987或当地标准/规范
	Refer to Japan Industry Standard

参照日本工业标准
	

	Stamping Profiles
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Note1: Standard wire gauges of American Wire Gauge: AWG, Birmingham Wire Gauge: BWG

Note2: The similar profile in Zinc coated, galvanized sheet and Aluminium- Zinc coated sheet

AZ150 Mean coated with a minimum 150gm of Alu-zinc compound per square-meter. Mean apply 75gm of Alu-zinc to each side total of 75x2=150 gm.

1：美国线规的标准线规：AWG，伯明翰线规：BWG

2：镀锌，镀锌板和镀铝锌板的类似外形

AZ150平均每平方米涂有最少150克铝锌复合物。 平均每边使用75克铝锌合计75x2 = 150克。
Color Coated Types，一年的采购数量：76,320
	Material photos
	Sr
	Specification
	Unit
	Remark

	Corrugated Iron sheet with multiple color bonded coating
多色涂层波纹铁皮板
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	1
	Material: Iron sheet with corrugated and color bond coating with zinc coat based (Galvanized Steel Sheet-G60) Multiple Colors available
材料：波纹状，彩色粘结涂层的锌铁基涂层（镀锌钢板-G60）多种颜色可供选择
	Minimum 0.60 oz. of Zinc per square-feet of coating as base coat
至少0.60盎司锌每平方英尺的涂层作为底漆
	Intl/local manufacture norm 
国际/本地制造规范

	
	2
	Base Sheet Thickness: 
30 Gauge: 0.3 mm or 0.012 inch

Tolerance: +/- 0.05mm

Tensile: High tensile steel
底板厚度：

30规格：0.3毫米或0.012英寸

公差：+/- 0.05mm

拉伸：高强度钢
	Gauge, millimeter
Minimum 550 Mpa strength
尺寸，毫米

最低550Mpa的强度
	AWG/BWG

	
	3
	Base zinc Coating Thickness in sides: 
Top: 5µm; Back: 5µm

Painting Thickness in sides:

Top: 18-20µm; Back: 5-7µm
底座锌涂层侧壁厚度：

顶部：5μm; 背面：5μm

侧面绘画厚度：

顶部：18-20μm; 背面：5-7μm
	0.30oz per square-feet in both sides coating micron unit for thickness
每平方英尺0.30盎司双面涂层微米单位的厚度
	Intl/local manufacture norm
国际/本地制造规范

	
	4
	Corrugated profile: 5 nos, Waves (normal)

Pitch: 200mm approx

Depth-height: 20mm approx

Tolerance: +/- 5 mm
波纹板外形：5号波浪（普通）？
间距：约200mm

深度 - 高度：约20毫米

公差：+/- 5毫米
	Qty of corrugated millimeter 
波峰单位为毫米（或英寸）
	Intl/local manufacture norm
国际/本地制造规范

	
	5
	Size of sheet: Width2.5 Feet (762 mm); Length: 7 Feet (2133mm) minimum (Tolerance width ±4mm, length ±15mm)
板材尺寸：宽度2.5英尺（762毫米）; 长度：最小7英尺（2133mm）（公差宽度±4mm，长度±15mm）
	Feet/inch or Meter/millimeter 
英尺/英寸或米/毫米
	Intl/local manufacture norm
国际/本地制造规范

	
	6
	Single sheet weight: () kg minimum Tolerance +/- 2%
单张重量：（kg）最小值公差+/- 2％
	Refer to manufactures
参考制造商
	Intl/local manufacture norm
国际/本地制造规范

	
	7
	Sheet Hardness HRB: 85HRB minimum

板材硬度HRB：最低85HRB
	Brinell Hardness Number. An abbreviation: e.g. 85 HRB

布氏硬度值。 缩写：例如 85 HRB
	Intl/local manufacture norm
国际/本地制造规范

	
	8
	Prefer standard: JIS G 3302-1987 or local standard/code

首选标准：JIS G 3302-1987或当地标准/规范
	Refer to Japan Industry Standard

参照日本工业标准
	International norm
国际制造规范

	Stamping Profiles

	[image: image6.png][ e

Corrugated







Note1: Standard wire gauges of American Wire Gauge: AWG, Birmingham Wire Gauge: BWG

Note2: Locally called as 4 angles sheets in market.

60 Galvanized Steel is hot dipped in zinc – coated with a minimum 0.60 oz. of zinc per square foot. Mean apply 0.30 oz. of zinc to each side total of 0.30x2=0.60 oz.
1：美国线规的标准线规：AWG，伯明翰线规：BWG

2：本地市场上称为4角钢板。

60镀锌钢热浸镀锌，最低0.60盎司锌每平方英尺。 符合0.30盎司锌每边总计0.30x2 = 0.60盎司。
Roofing Nail, 一年的采购数量：7,632
	S/n
	Description
	Length
	Form & Shank
	Diameter (Umbrella & shank)
	Washer
	Galvanizing
	Refer as Standard/Norm:

	1
	Used for roofing with Diamond form harden point anchor into purlin rail

带钻石形硬化锚点用于檩条轨道的屋顶
	3” (76 mm)

3英寸；76mm
	Umbrella Head with Smooth Shank or Plain shank

伞头平滑柄或平柄
	Head: 0.5” inch (approx: 14 mm) Shank: 0.120” inch (approx: 3.01 mm)

头部：0.5“英寸（约14mm）柄部：0.120”英寸（约3.01mm）
	Material of Plastic/Rubber

塑料/橡胶材料
	Hot dipping type

热浸式镀锌
	Material: Wire Rod BWG11: (Birmingham Wire Gauge)

材料：线材BWG11 :(伯明翰线规）


参考图片：（仅供参考）
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